{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":46,"n_cols":5,"rows_kept":46,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Ecolo-Tiger  875","Ecolo-Tiger 875, 9-Shank","Ecolo-Tiger 875, 11-Shank","Ecolo-Tiger 875, 13-Shank"]
["Dimensions And Weight"]
["Working Width ft-in","14ft","18ft","22ft","26ft"]
["Transport Width ft-in","16ft","16ft 9in","16ft 9in","18ft"]
["Overall Length ft-in","33ft 4in","33ft 4in","33ft 9in","33ft 9in"]
["Total Weight lb",14470,20000,25220,28200]
["Shanks"]
["Number Of Main Shanks ",7,9,11,13]
["Shank Spacing in",24,24,24,24]
["Shank Depth Adjustment Method ","Single-point depth control, crank","Single-point depth control, crank","Single-point depth control, crank","Single-point depth control, crank"]
["Optional Depth Adjustment Method ","AFS Soil Command, tractor console","AFS Soil Command, tractor console","AFS Soil Command, tractor console","AFS Soil Command, tractor console"]
["Standard Shank Design ","Parabolic, spring reset","Parabolic, spring reset","Parabolic, spring reset","Parabolic, spring reset"]
["Standard Shank Trip Force lb",3000,3000,3000,3000]
["Optional Shank Design ","Parabolic, shear bolt","Parabolic, shear bolt","Parabolic, shear bolt","Parabolic, shear bolt"]
["Underframe Clearance in",36.5,36.5,36.5,36.5]
["Shank Trip Clearance in",13,13,13,13]
["Disk, Forward Of Shanks"]
["Blade Type ","Disk","Disk","Disk","Disk"]
["Blade Diameter in",24,24,24,24]
["Blade Thickness in",0.26,0.26,0.26,0.26]
["Blade Spacing - in (mm) ","15 (381) w/ 24\" std; 12 (305) w/ 26\" opt.","15 (381) w/ 24\" std; 12 (305) w/ 26\" opt.","15 (381) w/ 24\" std; 12 (305) w/ 26\" opt.","15 (381) w/ 24\" std; 12 (305) w/ 26\" opt."]
["Blade Mounting ","Individual \"C\" hangers w/24\" std; gangs w/ 26\" opt","Individual \"C\" hangers w/24\" std; gangs w/ 26\" opt","Individual \"C\" hangers w/24\" std; gangs w/ 26\" opt","Individual \"C\" hangers w/24\" std; gangs w/ 26\" opt"]
["First Blade Angle Or Gang Angle - Degrees ",15,15,15,15]
["Second Blade Angle Or Gang Angle - Degrees ",15,15,15,15]
["Depth Adjustment ","Independent hydraulic disk depth control; AFS Soil Command optional","Independent hydraulic disk depth control; AFS Soil Command optional","Independent hydraulic disk depth control; AFS Soil Command optional","Independent hydraulic disk depth control; AFS Soil Command optional"]
["Rear Disk Behind Shanks"]
["Rear Blade Type ","Rear disk levelers to fill in shank path","Rear disk levelers to fill in shank path","Rear disk levelers to fill in shank path","Rear disk levelers to fill in shank path"]
["Rear Blade Diameter in",18,18,18,18]
["Rear Blade Spacing in",0,0,0,0]
["Rear Mounting ","Pairs","Pairs","Pairs","Pairs"]
["Rear Blade Angle Or Gang Angle - Degrees ","Opposing angles to level shank furrows","Opposing angles to level shank furrows","Opposing angles to level shank furrows","Opposing angles to level shank furrows"]
["Optional Attachments"]
["Rolling Reel / Basket ","Hydraulic double edge reel, optional","Hydraulic double edge reel, optional","Hydraulic double edge reel, optional","Hydraulic double edge reel, optional"]
["Spike Harrow ","Optional","Optional","Optional","Optional"]
["Coil Tine Harrow ","Optional","Optional","Optional","Optional"]
["Rear Hitch ","No","No","No","No"]
["Other Optional Attachment ","No","No","No","No"]
["Configuration, Frame And Hitch"]
["Sequence Of Tools ","Disk-Disk-Shanks-Leveler Disks","Disk-Disk-Shanks-Leveler Disks","Disk-Disk-Shanks-Leveler Disks","Disk-Disk-Shanks-Leveler Disks"]
["Manufacturer's Description Of Machine ","Disk Ripper","Disk Ripper","Disk Ripper","Disk Ripper"]
["Frame Type ","Non-folding","Folding","Folding","Folding"]
["Pull Type Hitch System ","Constant level hitch, adjustable","Constant level hitch, adjustable","Constant level hitch, adjustable","Constant level hitch, adjustable"]
["Tires And Wheel Mounting"]
["Transport Wheel Mounting ","Single","Single","Walking tandem","Walking tandem"]
["Transport Tyre Size ","425/65 R22.5","425/65 R22.5","16.5Lx16.1","16.5Lx16.1"]