{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":2,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","FARMALL 100A"]
["ENGINE"]
["FPT - EU Stage V [Hi-eSCR2]<br class=\"t-last-br\" />","✓"]
["Rated power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","74 / 100"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","4 / 3,600"]
["Max torque [Nm]<br class=\"t-last-br\" />","450 @ 1,300 rpm"]
["Torque rise [%]<br class=\"t-last-br\" />",47]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","130 / 14"]
["TRANSMISSION"]
["12x12 ManualDrive - with Powershuttle, 40 kph, optional creeper<br class=\"t-last-br\" />","✓"]
["HYDRAULICS"]
["Open Center pump - 82 l/min<br class=\"t-last-br\" />","✓"]
["Up to 3 mechanical rear remotes valves<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Mechanical mid mounts, incl. joystick for frontloader<br class=\"t-last-br\" />",2]
["PTO"]
["540/540E/1,000 @ 1,938/1,535/1,926 rpm<br class=\"t-last-br\" />","✓"]
["Electro-hydraulic activation<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["REAR LINKAGE"]
["MDC mechanical draft control Lift-O-Matic - max. lift capacity 4,400 kg<br class=\"t-last-br\" />","✓"]
["CONFIGURATION"]
["4-pillar cab with air conditioning, roof window, radio &amp; passenger seat<br class=\"t-last-br\" />","✓"]
["Mechanical front hitch with front PTO optional<br class=\"t-last-br\" />","✓"]
["Pneumatic trailer brake<br class=\"t-last-br\" />","✓"]
["FRONT LOADER CASE IH L3815A"]
["Mechanical self leveling,  FITLOCK2+ System&reg;- automatic hitching  incl. multi-connection,<br class=\"t-last-br\" />","✓"]
["SHOCK ELIMINATOR suspension, EURO implement carrier<br class=\"t-last-br\" />","✓"]
["3.80 m max. lift height @ implement pivot<br class=\"t-last-br\" />","✓"]
["1,650 kg max. payload 600 mm from implement pivot axis<br class=\"t-last-br\" />","✓"]