{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":28,"n_cols":2,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","FARMALL 75C ELECTRIC​"]
["ENGINE"]
["Rated power<br class=\"t-last-br\" />","55 kW / 75 hp"]
["Max torque","320 Nm​"]
["Max. capacity<br class=\"t-last-br\" />","110 kWh"]
["TRANSMISSION"]
["ManualDrive- 12x12 gears, electric Powershuttle, 40 kph<br class=\"t-last-br\" />","✓"]
["HYDRAULICS"]
["Open Center pump -  48 l/min<br class=\"t-last-br\" />","✓"]
["Up to 3 mechanical rear remote valves + Diverter<br class=\"t-last-br\" />","✓"]
["Mechanical mid-mounts, incl. Joystick for front loader<br class=\"t-last-br\" />",2]
["PTO"]
["540 / 540E&nbsp;<br class=\"t-last-br\" />","✓"]
["Electro-hydraulic PTO engagement<br class=\"t-last-br\" />","✓"]
["REAR LINKAGE"]
["MDC &ndash; mechanical draft control<br class=\"t-last-br\" />","✓"]
["Lift-O-Matic Plus<br class=\"t-last-br\" />","✓"]
["Max. lift capacity 2,750 kg","2,750 kg"]
["CONFIGURATION"]
["6-pillar cab incl. smart roof &amp; passenger seat<br class=\"t-last-br\" />","✓"]
["By wire Control - Powershuttle, Braking, PTO, Steering<br class=\"t-last-br\" />","✓"]
["AC-Charging &amp; DC Fast-Charging<br class=\"t-last-br\" />","✓"]
["Exportable Power- 230V outlets<br class=\"t-last-br\" />","✓"]
["FRONT LOADER CASE IH"]
["Mechanical self leveling<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["3.15 m max. lift height @ implement pivot<br class=\"t-last-br\" />","✓"]
["1,200 kg  max. payload 600 mm from implement pivot axis<br class=\"t-last-br\" />","✓"]